# REPORT — v0.170.0: root→Indítópult; gofmt normalization; stale-note; gate-denial check; SMART spike

**Date:** 2026-07-25 · **REPORT overwritten** (the standing rule; the prior append was a sanctioned one-off).

## 1. Baselines
| Repo | `main` @ start | version | → |
|------|----------------|---------|---|
| felhom-controller | `0a582ea` | v0.169.1 | v0.170.0 |
| felhom.eu | `e49f20f` | — | docs-only |

Re-verified clean at start.

## 2. Commits (feature commit NOT squashed with the gofmt commit — Scenario B)
- **`2487681`** — `style: gofmt normalization — no logic changes` (commit 1, style-only).
- **`9cc8424`** — `v0.170.0: root → Indítópult (302); Vezérlőpult at /dashboard; CLAUDE.md stale-note fix` (commit 2, feature).
- **felhom.eu `770ee5a`** — the SMART-coverage spike doc (+ nothing else).

## 3. Part 1 — Root → Indítópult
`server.go` route split: `"/"` → `http.Redirect(…"/launcher", 302)`; `"/dashboard"` keeps the handler.
`layout.html`: Vezérlőpult `href="/dashboard"` (topbar logo keeps `/` → redirects to launcher).
`auth.go` unchanged (post-login default `/` flows through the redirect to the launcher — verified).
Two dashboard-card tests repointed `/`→`/dashboard`.
- Tests (all pass): `TestRoot_RedirectsToLauncher` (302 + `Location: /launcher` + no launcher body at `/`),
  `TestDashboard_ServedAtDashboardURL` (200), `TestNav_LauncherAndDashboardHrefsAndActive`.
- **Red-proof (recorded):** fold `/` back into the dashboard case → `GET / status = 200, want 302` — FAIL, then restored.

## 4. Part 2 — gofmt normalization (46 files)
`gofmt -w` across the controller tree; `gofmt -l` now **empty**. Pure formatting: whitespace +
optional-semicolon removal in reflowed inline closures. **One caveat handled:** this system's Go-1.26
`gofmt` doc-comment reformatter rewrites `''`→`”` in doc comments; it hit exactly one comment
(`app_export_domain_test.go`, "yields ''") — reworded to "yields the empty string" so the result is
gofmt-clean without a garbled quote. Build+vet+test green before and after; separate prior commit.

## 5. Part 3 — CLAUDE.md stale note
Corrected the "vacation — agent DOWN at a remote site" block: felhom-pve is back on the home LAN, the
agent is **up** (`localapi` binds `192.168.0.162:8443`, `active`, capabilities 68/68), Tailscale alias
still available. (Inside the feature commit.)

## 6. Green gates + build/deploy
`go build ./... && go vet ./... && go test ./...` — **27 packages pass, 0 fail**; template/emoji/mojibake
gates OK. Built `felhom-controller:0.170.0`, deployed to guest 9201 → **Up (healthy)**,
`Controller elindult (0.170.0)`.

**Live (authed curl to `172.17.0.2:8080`, `Host: felhom.demo-felhom.eu`, login 302):**
- `GET /` → **302 → /launcher**.
- `GET /dashboard` → **200**, renders `<h2>Vezérlőpult</h2>`, nav `href="/dashboard" class="active"`.
- `GET /launcher` → **200**, nav `href="/launcher" class="active"`.

## 7. Part 4 — Quiesce gate-denial live check (v0.168.0 caveat)
**The v0.168.0 blocker (agent down) is GONE** — the agent is up and the gate is **code-live on 0.170.0**;
the quiesce loop is polling (`[quiesce] loop started (poll 5m0s…)`). **But the denial line is not
capturable right now**, for a *different* reason: the gate is only reached when a backup is **due**, and
the demo box is **within its cadence window** — `/backup/due` → `{"due":false,"reason":"within cadence
window","age_seconds":38260}` (~10.6 h since the last backup; default cadence `backup_cadence_seconds:0`
≈ 24 h). The debug ring (always-on for DEBUG) confirms **zero** quiesce gate lines. Also, "now"
(07:46 CEST) is *inside* the window `[04:30, 08:30)`, so even a due poll would ALLOW, not deny.

Forcing `due=true` would require changing the agent's `backup_cadence_seconds` — an **agent config
change, forbidden** by this task (read-only host). So the capture is **timing-gated**: the line will
emit on the next **due + outside-window** poll (next due ≈ this evening; any poll after `08:30` while
due denies). **The gate itself is fully unit-proven** (v0.168.0 Group D: outside→defer, safety-valve,
manual-never-gated). **Nothing was enabled or changed** — logging stays `info`, the window stays default
`02:30`; no restoration needed. *This is the one item I could not fully close in-session; it needs a
timed capture (operator, or a scheduled check) when the box is next due outside its window.*

## 8. Part 5 — SMART-coverage spike (findings-only, STOP)
Full doc: `felhom.eu/documentation/audits/SPIKE-smart-coverage-2026-07-25.md`. Read-only probes on
`demo-felhom` (a **real** N100, not virtualized). **Both physical disks report PASSED** via the exact
allowlisted `smartctl -a -j <dev>` (system SSD `sda` "AirDisk 512GB SSD"; USB HDD `sdb` "TOSHIBA
MQ04ABF100"). The card shows "Nincs adat" because the **agent never reads** them:
1. **`local` (system SSD) → UNKNOWN:** it's a `dir` on **LVM `pve-root`**; `backing_device` is empty and
   `smartDeviceFor` has **no dm/LVM branch**, so `/`→`pve-root`→`sda3`→`sda` is never resolved.
2. **USB `sdb` → ABSENT:** surfaced only via the **non-enriched `driveTargets.Known` union path** (sets
   `backing=/dev/sdb` but never calls `enrich`).

`-d sat` is **not needed** (the bridge passes SMART through with `-a -j`) and **not in sudoers** anyway
(only `-a -j /dev/sd[a-z]*` etc. are granted). The `by-uuid` symlink hypothesis doesn't apply (backing
is already the resolved `/dev/sdb`). **Graded fix directions (do-not-implement):** **B** — enrich the
union path (LOW risk, reaches the USB) **first**; **A** — dm/LVM resolution (MEDIUM risk, multi-PV care,
reaches the SYSTEM disk) **second**; **C** — `-d sat` + sudoers widening **rejected** (disproven here).
**STOP — no fix, no agent/sudoers/manifest change.**

## 9. Observations (out of scope)
- The `catchall.html` "Vezérlőpult" button uses `{{.ControllerURL}}` (the controller base URL) — it now
  lands on the launcher via the `/` redirect. A pre-existing label/destination nuance on a fallback page;
  left as-is (out of scope). Reword to "Indítópult" or point it at `/dashboard` in a future polish.
- The v0.170.0 image gives the whole disk-health feature a real-hardware home once the SMART-coverage
  fix (Part-5 directions) ships — the card will flip from "Nincs adat" to real PASSED verdicts.
